; 
; NXP  Communication Device Class driver installation file
; (C)2012 Copyright 
;

[Version] 
Signature="$Windows NT$" 
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318} 
Provider=%NXP% 
CatalogFile=lpc-composite-vcom.cat
DriverVer=09/12/2013,1.0.0.0

[Manufacturer] 
%NXP%=DeviceList, NTx86, NTamd64, NTARM

[DeviceList.NTx86] 
%DESCRIPTION%=LPCVCOM,USB\VID_1FC9&PID_0087 
%COMPOSITE%=LPCVCOM,USB\VID_1FC9&PID_0087&MI_01

[DeviceList.NTamd64] 
%DESCRIPTION%=LPCVCOM,USB\VID_1FC9&PID_0087 
%COMPOSITE%=LPCVCOM,USB\VID_1FC9&PID_0087&MI_01

[DeviceList.NTARM] 
%DESCRIPTION%=LPCVCOM,USB\VID_1FC9&PID_0087 
%COMPOSITE%=LPCVCOM,USB\VID_1FC9&PID_0087&MI_01

;------------------------------------------------------------------------------
;  Windows 2000/XP Sections
;------------------------------------------------------------------------------
[LPCVCOM]
include=mdmcpq.inf
CopyFiles=FakeModemCopyFileSection
AddReg=LowerFilterAddReg,SerialPropPageAddReg
[LPCVCOM.Services]
include = mdmcpq.inf
AddService = usbser, 0x00000002, LowerFilter_Service_Inst
; This adds the serial port property tab to the device properties dialog
[SerialPropPageAddReg]
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"
;------------------------------------------------------------------------------
;  String Definitions
;------------------------------------------------------------------------------

[Strings] 
NXP="NXP"
DESCRIPTION="LPC USB VCom Port" 
COMPOSITE="LPC USB VCom Port"



